10/11/06 Initially released.

10/11/06 Based on the datasheets using footprint supplied by International IR Rectifier.

01/14/08 Based on dated 02/19/07 SQ outline data sheet "IRF6712SPbF" footprint package height was increased to 27.4 mils.
