[Jumper Settings]
[The jumper shunts IPN#700000-842 should be installed
on only the headers with shunt information]

JUMPER    CONFIGURATION
------------------------------
J1A1      NO JUMPER SHUNT
J1A2      NO JUMPER SHUNT
J1A3      NO JUMPER SHUNT
J1A5      NO JUMPER SHUNT
J1A6      NO JUMPER SHUNT
J1H5      NO JUMPER SHUNT
J3A1      NO JUMPER SHUNT
J4J3      NO JUMPER SHUNT
J4K2      NO JUMPER SHUNT
J4K3      NO JUMPER SHUNT
J5K1      NO JUMPER SHUNT
J6K3      NO JUMPER SHUNT
J6K4      NO JUMPER SHUNT
J7K2      NO JUMPER SHUNT
J8K3      NO JUMPER SHUNT
J9B1      NO JUMPER SHUNT
J9B2      NO JUMPER SHUNT
J9C1      NO JUMPER SHUNT
J9E1      NO JUMPER SHUNT
J1A7      NO JUMPER SHUNT
J1B1      NO JUMPER SHUNT
J1K1      NO JUMPER SHUNT
J1B2      NO JUMPER SHUNT
J1F4      NO JUMPER SHUNT
J5A2      NO JUMPER SHUNT
J5B2      NO JUMPER SHUNT
J6D1      NO JUMPER SHUNT
J7D2      NO JUMPER SHUNT
J7E3      NO JUMPER SHUNT
J1E3      NO JUMPER SHUNT
J1F1      NO JUMPER SHUNT
J1F2      NO JUMPER SHUNT
J1F3      NO JUMPER SHUNT
J1F5      NO JUMPER SHUNT
J1F7      NO JUMPER SHUNT
J2H2      NO JUMPER SHUNT
J1G4      NO JUMPER SHUNT
J1G7      NO JUMPER SHUNT
J1H1      NO JUMPER SHUNT
J5A3      NO JUMPER SHUNT
J6E5      NO JUMPER SHUNT
J6E6      NO JUMPER SHUNT
J6F6      NO JUMPER SHUNT
J1H2      NO JUMPER SHUNT
J1J2      NO JUMPER SHUNT
J3A3      NO JUMPER SHUNT
J3J3      NO JUMPER SHUNT
J3J4      NO JUMPER SHUNT
J4A1      NO JUMPER SHUNT
J7D1      NO JUMPER SHUNT
J9C2      NO JUMPER SHUNT
J2J2      NO JUMPER SHUNT
J3D1      NO JUMPER SHUNT
J4J1      NO JUMPER SHUNT
J4J2      NO JUMPER SHUNT
J3J1      NO JUMPER SHUNT
J5B3      NO JUMPER SHUNT
J8D1      NO JUMPER SHUNT
J1A4      [1-2]     
J1E1      [1-2]     
J1E4      [1-2]     
J1H6      [1-2]     
J1J4      [1-2]     
J1J5      [1-2]     
J2J1      [1-2]     
J3A2      [1-2]     
J3F2      [1-2]     
J3J2      [1-2]     
J5F1      [1-2]     
J6E1      [1-2]     
J6E2      [1-2]     
J6E4      [1-2]     
J7C1      [1-2]     
J5C1      [2-3]     
J5C2      [2-3]     
J6C1      [2-3]     
J6K1      [2-3]     
J6K2      [2-3]     
J8K4      [2-3]     
J4K1      [1-2][3-4]
