%#################################################################
Title:        Cref Error Report
Design:       galileo
Date:         May 27 12:31:46 2014
%#################################################################



Warnings in Page : @galileo_lib.galileo(sch_1):Page5
Signal   PCIE0_TX0_N_C at (B 4) is labeled only once in the design.
Signal          RSVD_5 at (B 4) is labeled only once in the design.
Signal          RSVD_6 at (B 4) is labeled only once in the design.
Signal          RSVD_2 at (B 4) is labeled only once in the design.
Signal          RSVD_1 at (C 4) is labeled only once in the design.
Signal          RSVD_3 at (B 4) is labeled only once in the design.
Signal      DDR3_CMDPU at (C 4) is labeled only once in the design.
Signal       DDR3_DQPU at (C 4) is labeled only once in the design.
Signal      DDR3_ODTPU at (C 4) is labeled only once in the design.
Signal          RSVD_0 at (C 4) is labeled only once in the design.
Signal      PCIE_RBIAS at (B 6) is labeled only once in the design.
Signal   PCIE0_TX0_P_C at (B 4) is labeled only once in the design.
Signal          RSVD_4 at (B 4) is labeled only once in the design.
Signal     PCIE_IRCOMP at (B 4) is labeled only once in the design.

Warnings in Page : @galileo_lib.galileo(sch_1):Page6
Signal           RTCX2 at (B 8) is labeled only once in the design.
Signal EXT_REFCLK_HPLL at (A 3) is labeled only once in the design.
Signal           RTCX1 at (B 8) is labeled only once in the design.
Signal        RTCRST_N at (A 7) is labeled only once in the design.
Signal          PREQ_B at (C 2) is labeled only once in the design.
Signal          PRDY_B at (C 2) is labeled only once in the design.
Signal       MUX7_I0_R at (B 6) is labeled only once in the design.
Signal      LVL_C_A1_R at (C 6) is labeled only once in the design.
Signal       MUX0_I0_R at (C 6) is labeled only once in the design.
Signal     SPI1_MISO_R at (C 6) is labeled only once in the design.
Signal       MUX1_I0_R at (C 6) is labeled only once in the design.
Signal       MUX2_I0_R at (C 6) is labeled only once in the design.
Signal     SPI0_CS_N_R at (B 6) is labeled only once in the design.
Signal       MUX6_I0_R at (B 6) is labeled only once in the design.
Signal         GPIO3_R at (B 6) is labeled only once in the design.
Signal         RSVD_10 at (A 3) is labeled only once in the design.
Signal     SPI1_MOSI_R at (D 6) is labeled only once in the design.
Signal  RMII_REF_CLK_R at (A 3) is labeled only once in the design.
Signal     CLN_XTAL_IN at (B 3) is labeled only once in the design.
Signal       FLEX2_CLK at (B 3) is labeled only once in the design.
Signal       FLEX1_CLK at (B 3) is labeled only once in the design.
Signal       FLEX0_CLK at (B 3) is labeled only once in the design.
Signal    CLN_XTAL_OUT at (B 3) is labeled only once in the design.
Signal      SPI1_SCK_R at (C 6) is labeled only once in the design.
Signal      SPI0_SCK_R at (D 6) is labeled only once in the design.
Signal       VCCRTCEXT at (B 6) is labeled only once in the design.
Signal        OSC_COMP at (A 3) is labeled only once in the design.
Signal          RSVD_9 at (A 3) is labeled only once in the design.
Signal      CKSYS25OUT at (B 3) is labeled only once in the design.
Signal     SPI0_MOSI_R at (D 6) is labeled only once in the design.
Signal       MUX3_I0_R at (C 6) is labeled only once in the design.
Signal       MUX5_I0_R at (C 6) is labeled only once in the design.
Signal      LVL_C_A2_R at (C 6) is labeled only once in the design.
Signal       MUX8_I0_R at (C 6) is labeled only once in the design.
Signal      EXP2_INT_R at (B 6) is labeled only once in the design.
Signal  RTC32K_CLK_SEL at (B 6) is labeled only once in the design.
Signal          REF1_N at (B 3) is labeled only once in the design.
Signal          REF1_P at (B 3) is labeled only once in the design.
Signal          RSVD_8 at (B 3) is labeled only once in the design.
Signal          RSVD_7 at (B 3) is labeled only once in the design.
Signal             TP1 at (C 3) is labeled only once in the design.
Signal             TP0 at (C 3) is labeled only once in the design.

Warnings in Page : @galileo_lib.galileo(sch_1):Page7
Signal  RMII_S0_TXD0_R at (B 4) is labeled only once in the design.
Signal  RMII_S0_TXD1_R at (C 4) is labeled only once in the design.
Signal   RMII_S0_MDC_R at (B 4) is labeled only once in the design.
Signal  RMII_S0_MDIO_R at (B 4) is labeled only once in the design.
Signal         USBCOMP at (C 4) is labeled only once in the design.
Signal       TS_IREF_N at (D 7) is labeled only once in the design.
Signal    CLN_SD_CLK_R at (B 7) is labeled only once in the design.
Signal        PD_CLK14 at (C 7) is labeled only once in the design.
Signal         RSVD_12 at (C 4) is labeled only once in the design.
Signal         RSVD_11 at (C 4) is labeled only once in the design.
Signal       USB_OC1_N at (C 4) is labeled only once in the design.
Signal RMII_S0_TX_EN_R at (C 4) is labeled only once in the design.

Warnings in Page : @galileo_lib.galileo(sch_1):Page8
Signal      V1P5_S3_LC at (C 6) is labeled only once in the design.
Signal     V1P0_S5_IVR at (C 3) is labeled only once in the design.
Signal     V1P0_S0_FLT at (D 6) is labeled only once in the design.

Warnings in Page : @galileo_lib.galileo(sch_1):Page10
Signal            ZQ_1 at (B 5) is labeled only once in the design.

Warnings in Page : @galileo_lib.galileo(sch_1):Page11
Signal            ZQ_2 at (B 5) is labeled only once in the design.

Warnings in Page : @galileo_lib.galileo(sch_1):Page12
Signal        M_CK_CAP at (D 2) is labeled only once in the design.

Warnings in Page : @galileo_lib.galileo(sch_1):Page13
Signal        SLT0_SCL at (B 4) is labeled only once in the design.
Signal        SLT0_SDA at (B 4) is labeled only once in the design.

Warnings in Page : @galileo_lib.galileo(sch_1):Page14
Signal          LED_SD at (A 5) is labeled only once in the design.
Signal   CLN_SD_DAT3_R at (C 5) is labeled only once in the design.
Signal   CLN_SD_DAT0_R at (C 5) is labeled only once in the design.
Signal   CLN_SD_DAT1_R at (C 5) is labeled only once in the design.
Signal   CLN_SD_CD_N_R at (C 5) is labeled only once in the design.
Signal    CLN_SD_CMD_R at (C 5) is labeled only once in the design.
Signal   CLN_SD_DAT2_R at (C 5) is labeled only once in the design.

Warnings in Page : @galileo_lib.galileo(sch_1):Page15
Signal     USBH2_DN_CH at (A 4) is labeled only once in the design.
Signal     USBH2_DP_CH at (A 4) is labeled only once in the design.
Signal       LED_VBUS1 at (D 4) is labeled only once in the design.
Signal     USBH0_DN_CH at (C 3) is labeled only once in the design.
Signal     USBH0_DP_CH at (C 3) is labeled only once in the design.

Warnings in Page : @galileo_lib.galileo(sch_1):Page16
Signal   UART1_RTS_N_R at (C 3) is labeled only once in the design.
Signal     UART1_TXD_R at (C 3) is labeled only once in the design.
Signal UART1_RXD_MUX_R at (C 3) is labeled only once in the design.
Signal   UART1_CTS_N_R at (C 3) is labeled only once in the design.
Signal      JTAG_TMS_R at (A 7) is labeled only once in the design.
Signal      JTAG_TCK_R at (A 7) is labeled only once in the design.

Warnings in Page : @galileo_lib.galileo(sch_1):Page17
Signal        VPOE_ADJ at (A 7) is labeled only once in the design.
Signal     RMII_S0_CT1 at (A 3) is labeled only once in the design.
Signal     LED_RJ45_C2 at (A 2) is labeled only once in the design.
Signal      RMII_VC3_R at (A 3) is labeled only once in the design.
Signal     LED_RJ45_C1 at (A 2) is labeled only once in the design.
Signal      RMII_VC2_R at (A 3) is labeled only once in the design.
Signal      RMII_VC1_R at (A 3) is labeled only once in the design.
Signal      RMII_VC4_R at (A 3) is labeled only once in the design.
Signal       PHY_RBIAS at (C 4) is labeled only once in the design.
Signal       ETH_BLINK at (C 3) is labeled only once in the design.
Signal  RMII_S0_RXD0_R at (C 3) is labeled only once in the design.
Signal  RMII_S0_RXD1_R at (C 3) is labeled only once in the design.

Warnings in Page : @galileo_lib.galileo(sch_1):Page18
Signal     ANALOG_A1_R at (A 5) is labeled only once in the design.
Signal     ANALOG_A2_R at (A 5) is labeled only once in the design.
Signal     SPI0_MISO_R at (A 3) is labeled only once in the design.
Signal     ANALOG_A3_R at (A 5) is labeled only once in the design.
Signal         AVIN4_R at (A 5) is labeled only once in the design.
Signal         AVIN5_R at (A 5) is labeled only once in the design.
Signal     ANALOG_A0_R at (A 5) is labeled only once in the design.
Signal       VCC_FLASH at (D 6) is labeled only once in the design.
Signal     LSPI_MISO_R at (C 3) is labeled only once in the design.
Signal        LSPI_SCK at (C 4) is labeled only once in the design.
Signal       AT25_WP_N at (C 4) is labeled only once in the design.
Signal       LSPI_CS_N at (C 4) is labeled only once in the design.
Signal       LSPI_MOSI at (C 4) is labeled only once in the design.
Signal     AT25_HOLD_N at (C 4) is labeled only once in the design.
Signal    VCC_DEDIPROG at (D 8) is labeled only once in the design.
Signal   V5_ALW_ON_FIL at (B 4) is labeled only once in the design.

Warnings in Page : @galileo_lib.galileo(sch_1):Page20
Signal        EXP1_INT at (C 4) is labeled only once in the design.
Signal        EXP0_INT at (D 6) is labeled only once in the design.
Signal      ANALOG_A0R at (B 6) is labeled only once in the design.
Signal      ANALOG_A1R at (B 6) is labeled only once in the design.
Signal      ANALOG_A2R at (B 6) is labeled only once in the design.
Signal      ANALOG_A3R at (B 6) is labeled only once in the design.
Signal     AMUX2_NO1_R at (B 6) is labeled only once in the design.
Signal     AMUX2_NO2_R at (B 6) is labeled only once in the design.
Signal         MUX_IO2 at (B 6) is labeled only once in the design.
Signal         MUX_IO3 at (B 6) is labeled only once in the design.

Warnings in Page : @galileo_lib.galileo(sch_1):Page22
Signal         BUF_IO3 at (C 7) is labeled only once in the design.
Signal         BUF_IO5 at (C 7) is labeled only once in the design.
Signal         BUF_IO6 at (C 7) is labeled only once in the design.
Signal         BUF_IO9 at (C 7) is labeled only once in the design.
Signal        BUF_IO11 at (B 7) is labeled only once in the design.
Signal        BUF_IO10 at (B 7) is labeled only once in the design.
Signal         BUF_IO1 at (B 7) is labeled only once in the design.
Signal     LVL_B_OE5_N at (B 7) has too little display space.
Signal     LVL_B_OE4_N at (B 7) has too little display space.

Warnings in Page : @galileo_lib.galileo(sch_1):Page23
Signal   BUF_SPI1_MISO at (B 3) is labeled only once in the design.
Signal      IO13_LED_R at (B 6) is labeled only once in the design.
Signal         BUF_IO0 at (C 6) is labeled only once in the design.
Signal         BUF_IO2 at (C 6) is labeled only once in the design.
Signal         BUF_IO4 at (C 6) is labeled only once in the design.
Signal        BUF_IO12 at (B 6) is labeled only once in the design.
Signal        IO13_LED at (B 6) is labeled only once in the design.

Warnings in Page : @galileo_lib.galileo(sch_1):Page24
Signal     IO11_ICSP_R at (A 3) is labeled only once in the design.
Signal      AMUX2_COM2 at (C 6) is labeled only once in the design.
Signal            AREF at (D 2) is labeled only once in the design.
Signal          IO10_R at (D 2) is labeled only once in the design.
Signal          IO12_R at (D 2) is labeled only once in the design.
Signal          IO11_R at (D 2) is labeled only once in the design.
Signal          IO13_R at (D 2) is labeled only once in the design.
Signal           IO9_R at (D 2) is labeled only once in the design.
Signal           IO6_R at (C 2) is labeled only once in the design.
Signal           IO5_R at (C 2) is labeled only once in the design.
Signal           IO0_R at (C 2) is labeled only once in the design.
Signal           IO2_R at (C 2) is labeled only once in the design.
Signal           IO3_R at (C 2) is labeled only once in the design.
Signal           IO1_R at (C 2) is labeled only once in the design.
Signal           IO4_R at (C 2) is labeled only once in the design.
Signal     IO13_ICSP_R at (A 4) is labeled only once in the design.
Signal     IO12_ICSP_R at (A 4) is labeled only once in the design.
Signal      AMUX2_COM1 at (C 6) is labeled only once in the design.

Warnings in Page : @galileo_lib.galileo(sch_1):Page25
Signal           SS1_1 at (C 6) is labeled only once in the design.
Signal         RLIM1_1 at (C 6) is labeled only once in the design.
Signal         RLIM1_3 at (B 6) is labeled only once in the design.
Signal         RLIM1_2 at (C 6) is labeled only once in the design.
Signal          BST1_3 at (B 6) is labeled only once in the design.
Signal     VR1_COMP1_R at (A 8) is labeled only once in the design.
Signal     VR1_COMP2_R at (A 7) is labeled only once in the design.
Signal          BST1_1 at (C 6) is labeled only once in the design.
Signal           SS1_2 at (C 6) is labeled only once in the design.
Signal          BST1_2 at (B 6) is labeled only once in the design.
Signal           SS1_3 at (B 6) is labeled only once in the design.
Signal         ROSC_VR at (B 5) is labeled only once in the design.
Signal           F_PWM at (B 5) is labeled only once in the design.
Signal             V7V at (C 4) is labeled only once in the design.
Signal             V3V at (C 4) is labeled only once in the design.
Signal     VR1_COMP3_R at (A 6) is labeled only once in the design.

Warnings in Page : @galileo_lib.galileo(sch_1):Page27
Signal USB_PWR_FAULT_N at (C 3) is labeled only once in the design.
Signal     V5_ALW_ON_L at (B 2) is labeled only once in the design.
Signal   REFIN_VTT_REG at (C 8) is labeled only once in the design.
Signal     V5_ALW_ON_D at (B 1) is labeled only once in the design.
Signal    PG_3P3_S5_NU at (D 5) is labeled only once in the design.
Signal    PG_V5_ALW_ON at (B 2) is labeled only once in the design.
Signal    FB_V5_ALW_ON at (B 2) is labeled only once in the design.
Signal           VIN_D at (B 4) is labeled only once in the design.

Warnings in Page : @galileo_lib.galileo(sch_1):Page28
Signal         BAT_POS at (A 3) is labeled only once in the design.
Signal         BAT_DIO at (A 3) is labeled only once in the design.
Signal   S0_1V0_EN_LED at (C 4) is labeled only once in the design.
