(Pinlist
	(Pin
		(Name A2)
		(MSB )
		(LSB )
		(Type INPUT)
		(Location Left)
		(InputLoadLow -0.01)
		(InputLoadHigh 0.01)
		(OutputLoadLow )
		(OutputLoadHigh )
		(CheckLoad Both)
		(CheckIO Both)
		(CheckDir 1)
		(CheckAssert 1)
		(CheckOutput 1)
		(UnknownLoading 0)
		(PinShape )
		(DIFF_PAIR_PINS_POS )
		(DIFF_PAIR_PINS_NEG )
	)

	(Pin
		(Name A1)
		(MSB )
		(LSB )
		(Type INPUT)
		(Location Left)
		(InputLoadLow -0.01)
		(InputLoadHigh 0.01)
		(OutputLoadLow )
		(OutputLoadHigh )
		(CheckLoad Both)
		(CheckIO Both)
		(CheckDir 1)
		(CheckAssert 1)
		(CheckOutput 1)
		(UnknownLoading 0)
		(PinShape )
		(DIFF_PAIR_PINS_POS )
		(DIFF_PAIR_PINS_NEG )
	)

	(Pin
		(Name VDD)
		(MSB )
		(LSB )
		(Type POWER)
		(Location Top)
		(InputLoadLow )
		(InputLoadHigh )
		(OutputLoadLow )
		(OutputLoadHigh )
		(CheckLoad Off)
		(CheckIO Off)
		(CheckDir 0)
		(CheckAssert 0)
		(CheckOutput 0)
		(UnknownLoading 0)
		(PinShape )
		(DIFF_PAIR_PINS_POS )
		(DIFF_PAIR_PINS_NEG )
	)

	(Pin
		(Name A0)
		(MSB )
		(LSB )
		(Type INPUT)
		(Location Left)
		(InputLoadLow -0.01)
		(InputLoadHigh 0.01)
		(OutputLoadLow )
		(OutputLoadHigh )
		(CheckLoad Both)
		(CheckIO Both)
		(CheckDir 1)
		(CheckAssert 1)
		(CheckOutput 1)
		(UnknownLoading 0)
		(PinShape )
		(DIFF_PAIR_PINS_POS )
		(DIFF_PAIR_PINS_NEG )
	)

	(Pin
		(Name P1_7)
		(MSB )
		(LSB )
		(Type BIDIR)
		(Location Right)
		(InputLoadLow -0.01)
		(InputLoadHigh 0.01)
		(OutputLoadLow 1.0)
		(OutputLoadHigh -1.0)
		(CheckLoad Both)
		(CheckIO Both)
		(CheckDir 1)
		(CheckAssert 1)
		(CheckOutput 1)
		(UnknownLoading 0)
		(PinShape )
		(DIFF_PAIR_PINS_POS )
		(DIFF_PAIR_PINS_NEG )
	)

	(Pin
		(Name P1_6)
		(MSB )
		(LSB )
		(Type BIDIR)
		(Location Right)
		(InputLoadLow -0.01)
		(InputLoadHigh 0.01)
		(OutputLoadLow 1.0)
		(OutputLoadHigh -1.0)
		(CheckLoad Both)
		(CheckIO Both)
		(CheckDir 1)
		(CheckAssert 1)
		(CheckOutput 1)
		(UnknownLoading 0)
		(PinShape )
		(DIFF_PAIR_PINS_POS )
		(DIFF_PAIR_PINS_NEG )
	)

	(Pin
		(Name P1_5)
		(MSB )
		(LSB )
		(Type BIDIR)
		(Location Right)
		(InputLoadLow -0.01)
		(InputLoadHigh 0.01)
		(OutputLoadLow 1.0)
		(OutputLoadHigh -1.0)
		(CheckLoad Both)
		(CheckIO Both)
		(CheckDir 1)
		(CheckAssert 1)
		(CheckOutput 1)
		(UnknownLoading 0)
		(PinShape )
		(DIFF_PAIR_PINS_POS )
		(DIFF_PAIR_PINS_NEG )
	)

	(Pin
		(Name P1_4)
		(MSB )
		(LSB )
		(Type BIDIR)
		(Location Right)
		(InputLoadLow -0.01)
		(InputLoadHigh 0.01)
		(OutputLoadLow 1.0)
		(OutputLoadHigh -1.0)
		(CheckLoad Both)
		(CheckIO Both)
		(CheckDir 1)
		(CheckAssert 1)
		(CheckOutput 1)
		(UnknownLoading 0)
		(PinShape )
		(DIFF_PAIR_PINS_POS )
		(DIFF_PAIR_PINS_NEG )
	)

	(Pin
		(Name P1_3)
		(MSB )
		(LSB )
		(Type BIDIR)
		(Location Right)
		(InputLoadLow -0.01)
		(InputLoadHigh 0.01)
		(OutputLoadLow 1.0)
		(OutputLoadHigh -1.0)
		(CheckLoad Both)
		(CheckIO Both)
		(CheckDir 1)
		(CheckAssert 1)
		(CheckOutput 1)
		(UnknownLoading 0)
		(PinShape )
		(DIFF_PAIR_PINS_POS )
		(DIFF_PAIR_PINS_NEG )
	)

	(Pin
		(Name P1_2)
		(MSB )
		(LSB )
		(Type BIDIR)
		(Location Right)
		(InputLoadLow -0.01)
		(InputLoadHigh 0.01)
		(OutputLoadLow 1.0)
		(OutputLoadHigh -1.0)
		(CheckLoad Both)
		(CheckIO Both)
		(CheckDir 1)
		(CheckAssert 1)
		(CheckOutput 1)
		(UnknownLoading 0)
		(PinShape )
		(DIFF_PAIR_PINS_POS )
		(DIFF_PAIR_PINS_NEG )
	)

	(Pin
		(Name P1_1)
		(MSB )
		(LSB )
		(Type BIDIR)
		(Location Right)
		(InputLoadLow -0.01)
		(InputLoadHigh 0.01)
		(OutputLoadLow 1.0)
		(OutputLoadHigh -1.0)
		(CheckLoad Both)
		(CheckIO Both)
		(CheckDir 1)
		(CheckAssert 1)
		(CheckOutput 1)
		(UnknownLoading 0)
		(PinShape )
		(DIFF_PAIR_PINS_POS )
		(DIFF_PAIR_PINS_NEG )
	)

	(Pin
		(Name P1_0)
		(MSB )
		(LSB )
		(Type BIDIR)
		(Location Right)
		(InputLoadLow -0.01)
		(InputLoadHigh 0.01)
		(OutputLoadLow 1.0)
		(OutputLoadHigh -1.0)
		(CheckLoad Both)
		(CheckIO Both)
		(CheckDir 1)
		(CheckAssert 1)
		(CheckOutput 1)
		(UnknownLoading 0)
		(PinShape )
		(DIFF_PAIR_PINS_POS )
		(DIFF_PAIR_PINS_NEG )
	)

	(Pin
		(Name VSS)
		(MSB )
		(LSB )
		(Type GROUND)
		(Location Top)
		(InputLoadLow )
		(InputLoadHigh )
		(OutputLoadLow )
		(OutputLoadHigh )
		(CheckLoad Off)
		(CheckIO Off)
		(CheckDir 0)
		(CheckAssert 0)
		(CheckOutput 0)
		(UnknownLoading 0)
		(PinShape )
		(DIFF_PAIR_PINS_POS )
		(DIFF_PAIR_PINS_NEG )
	)

	(Pin
		(Name P0_7)
		(MSB )
		(LSB )
		(Type BIDIR)
		(Location Right)
		(InputLoadLow -0.01)
		(InputLoadHigh 0.01)
		(OutputLoadLow 1.0)
		(OutputLoadHigh -1.0)
		(CheckLoad Both)
		(CheckIO Both)
		(CheckDir 1)
		(CheckAssert 1)
		(CheckOutput 1)
		(UnknownLoading 0)
		(PinShape )
		(DIFF_PAIR_PINS_POS )
		(DIFF_PAIR_PINS_NEG )
	)

	(Pin
		(Name P0_6)
		(MSB )
		(LSB )
		(Type BIDIR)
		(Location Right)
		(InputLoadLow -0.01)
		(InputLoadHigh 0.01)
		(OutputLoadLow 1.0)
		(OutputLoadHigh -1.0)
		(CheckLoad Both)
		(CheckIO Both)
		(CheckDir 1)
		(CheckAssert 1)
		(CheckOutput 1)
		(UnknownLoading 0)
		(PinShape )
		(DIFF_PAIR_PINS_POS )
		(DIFF_PAIR_PINS_NEG )
	)

	(Pin
		(Name P0_5)
		(MSB )
		(LSB )
		(Type BIDIR)
		(Location Right)
		(InputLoadLow -0.01)
		(InputLoadHigh 0.01)
		(OutputLoadLow 1.0)
		(OutputLoadHigh -1.0)
		(CheckLoad Both)
		(CheckIO Both)
		(CheckDir 1)
		(CheckAssert 1)
		(CheckOutput 1)
		(UnknownLoading 0)
		(PinShape )
		(DIFF_PAIR_PINS_POS )
		(DIFF_PAIR_PINS_NEG )
	)

	(Pin
		(Name P0_4)
		(MSB )
		(LSB )
		(Type BIDIR)
		(Location Right)
		(InputLoadLow -0.01)
		(InputLoadHigh 0.01)
		(OutputLoadLow 1.0)
		(OutputLoadHigh -1.0)
		(CheckLoad Both)
		(CheckIO Both)
		(CheckDir 1)
		(CheckAssert 1)
		(CheckOutput 1)
		(UnknownLoading 0)
		(PinShape )
		(DIFF_PAIR_PINS_POS )
		(DIFF_PAIR_PINS_NEG )
	)

	(Pin
		(Name P0_3)
		(MSB )
		(LSB )
		(Type BIDIR)
		(Location Right)
		(InputLoadLow -0.01)
		(InputLoadHigh 0.01)
		(OutputLoadLow 1.0)
		(OutputLoadHigh -1.0)
		(CheckLoad Both)
		(CheckIO Both)
		(CheckDir 1)
		(CheckAssert 1)
		(CheckOutput 1)
		(UnknownLoading 0)
		(PinShape )
		(DIFF_PAIR_PINS_POS )
		(DIFF_PAIR_PINS_NEG )
	)

	(Pin
		(Name P0_2)
		(MSB )
		(LSB )
		(Type BIDIR)
		(Location Right)
		(InputLoadLow -0.01)
		(InputLoadHigh 0.01)
		(OutputLoadLow 1.0)
		(OutputLoadHigh -1.0)
		(CheckLoad Both)
		(CheckIO Both)
		(CheckDir 1)
		(CheckAssert 1)
		(CheckOutput 1)
		(UnknownLoading 0)
		(PinShape )
		(DIFF_PAIR_PINS_POS )
		(DIFF_PAIR_PINS_NEG )
	)

	(Pin
		(Name P0_1)
		(MSB )
		(LSB )
		(Type BIDIR)
		(Location Right)
		(InputLoadLow -0.01)
		(InputLoadHigh 0.01)
		(OutputLoadLow 1.0)
		(OutputLoadHigh -1.0)
		(CheckLoad Both)
		(CheckIO Both)
		(CheckDir 1)
		(CheckAssert 1)
		(CheckOutput 1)
		(UnknownLoading 0)
		(PinShape )
		(DIFF_PAIR_PINS_POS )
		(DIFF_PAIR_PINS_NEG )
	)

	(Pin
		(Name INT_N)
		(MSB )
		(LSB )
		(Type OUTPUT)
		(Location Right)
		(InputLoadLow )
		(InputLoadHigh )
		(OutputLoadLow 1.0)
		(OutputLoadHigh -1.0)
		(CheckLoad Both)
		(CheckIO Both)
		(CheckDir 1)
		(CheckAssert 1)
		(CheckOutput 1)
		(UnknownLoading 0)
		(PinShape )
		(DIFF_PAIR_PINS_POS )
		(DIFF_PAIR_PINS_NEG )
	)

	(Pin
		(Name SDA)
		(MSB )
		(LSB )
		(Type BIDIR)
		(Location Right)
		(InputLoadLow -0.01)
		(InputLoadHigh 0.01)
		(OutputLoadLow 1.0)
		(OutputLoadHigh -1.0)
		(CheckLoad Both)
		(CheckIO Both)
		(CheckDir 1)
		(CheckAssert 1)
		(CheckOutput 1)
		(UnknownLoading 0)
		(PinShape )
		(DIFF_PAIR_PINS_POS )
		(DIFF_PAIR_PINS_NEG )
	)

	(Pin
		(Name SCL)
		(MSB )
		(LSB )
		(Type INPUT)
		(Location Left)
		(InputLoadLow -0.01)
		(InputLoadHigh 0.01)
		(OutputLoadLow )
		(OutputLoadHigh )
		(CheckLoad Both)
		(CheckIO Both)
		(CheckDir 1)
		(CheckAssert 1)
		(CheckOutput 1)
		(UnknownLoading 0)
		(PinShape )
		(DIFF_PAIR_PINS_POS )
		(DIFF_PAIR_PINS_NEG )
	)

	(Pin
		(Name P0_0)
		(MSB )
		(LSB )
		(Type BIDIR)
		(Location Right)
		(InputLoadLow -0.01)
		(InputLoadHigh 0.01)
		(OutputLoadLow 1.0)
		(OutputLoadHigh -1.0)
		(CheckLoad Both)
		(CheckIO Both)
		(CheckDir 1)
		(CheckAssert 1)
		(CheckOutput 1)
		(UnknownLoading 0)
		(PinShape )
		(DIFF_PAIR_PINS_POS )
		(DIFF_PAIR_PINS_NEG )
	)

	(Pin
		(Name THPAD)
		(MSB )
		(LSB )
		(Type GROUND)
		(Location Top)
		(InputLoadLow )
		(InputLoadHigh )
		(OutputLoadLow )
		(OutputLoadHigh )
		(CheckLoad Off)
		(CheckIO Off)
		(CheckDir 0)
		(CheckAssert 0)
		(CheckOutput 0)
		(UnknownLoading 0)
		(PinShape )
		(DIFF_PAIR_PINS_POS )
		(DIFF_PAIR_PINS_NEG )
	)


)